AY-3-8910 To Do
---------------

	Should compare against current frequency value instead of counting
	from frequency value to zero.
	Envelope frequency should be able to go lower (0 = half of 1, is this only on YM2149?).
	Save more info of state.
