READMEBO.TXT -- information about ADAMserve boot disk images
by Richard F. Drushel  drushel@apk.net  13 August 2000


(1) ADAMserve Boot Disk Images.

The following 160K disk images are provided for booting ADAMserve:

    ASBOOT16.IMG    ;Micro Innovations port 2
    ASBOOT24.IMG    ;Micro Innovations port 1
    ASBOOT68.IMG    ;Eve/Orphanware port 44H
    ASBOOT76.IMG    ;Orphanware port 4CH
    ASBOOT84.IMG    ;Orphanware port 54H
    ASBOOT92.IMG    ;Orphanware port 5CH

These images are identical except for the serial baseport byte at offset 2
(0-based).  They contain:

    the ADAMserve boot block
    the ADAMserve HARDDISK boot block
    ADAMserve HARDDISK 4.203
    EOS4.0
    EOS4.X
    File Manager 4.1

These images may be cloned to actual 160K disks using the appropriate TDOS
program, CLONE.COM.  They could also be block-copied onto disks starting from
block 0, using File Manager and a source medium which is bigger than 160K.
Only the first 47 blocks (blocks 0-46) actually have data on them, however, so
it is possible to transfer less than the full 160 blocks.  Though disk images,
they may also be copied to tape for boot purposes; ADAMserve won't care.


(2) Usage.

For complete instructions, see README72.TXT.


--RFD


