This memory card can be configured for 64KB, 128KB, 192KB or 256KB. It was only sold in 64KB and 256KB configurations and in order for the ADAM to recognize 256K of expanded memory, an Addressor Card (installed in Slot #2) is required.
