Next: 4.6.15 Interrupts Up: 4.6 The PIC16 port Previous: 4.6.13 Functions Contents Index

## 4.6.14 Function return values

Return values from functions are placed to the appropriate registers following a modified Microchip policy optimized for SDCC. The following table shows these registers:

size | destination register
8 bits | WREG
16 bits | PRODL:WREG
24 bits | PRODH:PRODL:WREG
32 bits | FSR0L:PRODH:PRODL:WREG
>32 bits | on stack, FSR0 points to the beginning