Next: 3.17.3 Math functions (sinf, Up: 3.17 Library Routines Previous: 3.17.1 Compiler support routines Contents Index
Subsections

- 3.17.2.1 <stdio.h>
  - 3.17.2.1.1 getchar(), putchar()
  - 3.17.2.1.2 printf()
- 3.17.2.2 <malloc.h>

## 3.17.2 Stdclib functions (puts, printf, strcat etc.)

### 3.17.2.1 <stdio.h>

#### 3.17.2.1.1 getchar(), putchar()

As usual on embedded systems you have to provide your own `getchar()` and `putchar()` routines. SDCC does not know whether the system connects to a serial line with or without handshake, LCD, keyboard or other device. And whether a `lf` to `crlf` conversion within `putchar()` is intended. You'll find examples for serial routines f.e. in sdcc/device/lib. For the mcs51 this minimalistic polling `putchar()` routine might be a start:

> `void putchar (char c) {`
> `while (!TI) /* assumes UART is initialized */`
> `;`
> `TI = 0;`
> `SBUF = c;`
> `}`

#### 3.17.2.1.2 printf()

The default `printf()` implementation in `printf_large.c` does not support float (except on ds390), only <NO FLOAT> will be printed instead of the value. To enable floating point output, recompile it with the option -DUSE_FLOATS=1 on the command line. Use --model-large for the mcs51 port, since this uses a lot of memory. To enable float support for the pic16 targets, see 4.6.9.

If you're short on code memory you might want to use `printf_small()` instead of `printf().` For the mcs51 there additionally are assembly versions `printf_tiny()` (subset of printf using less than 270 bytes) and `printf_fast()` and `printf_fast_f()` (floating-point aware version of printf_fast) which should fit the requirements of many embedded systems (printf_fast() can be customized by unsetting #defines to not support long variables and field widths). Be sure to use only one of these printf options within a project.

Feature matrix of different printf options on mcs51.

mcs51 | printf | printf USE_FLOATS=1 | printf_small | printf_fast | printf_fast_f | printf_tiny
filename | printf_large.c | printf_large.c | printfl.c | printf_fast.c | printf_fast_f.c | printf_tiny.c
''Hello World'' size small / large | 1.7k / 2.4k | 4.3k / 5.6k | 1.2k / 1.8k | 1.3k / 1.3k | 1.9k / 1.9k | 0.44k / 0.44k
code size small / large | 1.4k / 2.0k | 2.8k / 3.7k | 0.45k / 0.47k (+ _ltoa) | 1.2k / 1.2k | 1.6k / 1.6k | 0.26k / 0.26k
formats | cdiopsux | cdfiopsux | cdosx | cdsux | cdfsux | cdsux
long (32 bit) support | x | x | x | x | x | -
byte arguments on stack | b | b | - | - | - | -
float format | - | %f | - | - | %f3.10 | -
float formats %e %g | - | - | - | - | - | -
field width | x | x | - | x | x | -
string speed3.11, small / large | 1.52 / 2.59 ms | 1.53 / 2.62 ms | 0.92 / 0.93 ms | 0.45 / 0.45 ms | 0.46 / 0.46 ms | 0.45 / 0.45 ms
int speed3.12, small / large | 3.01 / 3.61 ms | 3.01 / 3.61 ms | 3.51 / 18.13 ms | 0.22 / 0.22 ms | 0.23 / 0.23 ms | 0.25 / 0.25 ms3.13
long speed3.14, small / large | 5.37 / 6.31 ms | 5.37 / 6.31 ms | 8.71 / 40.65 ms | 0.40 / 0.40 ms | 0.40 / 0.40 ms | -
float speed3.15, small / large | - | 7.49 / 22.47 ms | - | - | 1.04 / 1.04 ms | -

###
3.17.2.2 <malloc.h>

As of SDCC 2.6.2 you no longer need to call an initialization routine before using dynamic memory allocation and a default heap space of 1024 bytes is provided for malloc to allocate memory from. If you need a different heap size you need to recompile _heap.c with the required size defined in HEAP_SIZE. It is recommended to make a copy of this file into your project directory and compile it there with:

> `sdcc -c _heap.c -D HEAP_SIZE=2048`

And then link it with:

> `sdcc main.rel _heap.rel`

Next: 3.17.3 Math functions (sinf, Up: 3.17 Library Routines Previous: 3.17.1 Compiler support routines Contents Index