Next: 1.2 Open Source Up: 1. Introduction Previous: 1. Introduction Contents Index

# 1.1 About SDCC

SDCC (Small Device C Compiler) is free open source, retargettable, optimizing ANSI-C compiler by Sandeep Dutta designed for 8 bit Microprocessors. The current version targets Intel MCS51 based Microprocessors (8031, 8032, 8051, 8052, etc.), Dallas DS80C390 variants, Freescale (formerly Motorola) HC08 and Zilog Z80 based MCUs. It can be retargeted for other microprocessors, support for Microchip PIC is under development. The entire source code for the compiler is distributed under GPL. SDCC uses a modified version of ASXXXX & ASLINK, free open source retargetable assembler & linker. SDCC has extensive language extensions suitable for utilizing various microcontrollers and underlying hardware effectively.
In addition to the MCU specific optimizations SDCC also does a host of standard optimizations like:

- global sub expression elimination,
- loop optimizations (loop invariant, strength reduction of induction variables and loop reversing),
- constant folding & propagation,
- copy propagation,
- dead code elimination
- jump tables for switch statements.

For the back-end SDCC uses a global register allocation scheme which should be well suited for other 8 bit MCUs.
The peep hole optimizer uses a rule based substitution mechanism which is MCU independent.
Supported data-types are:

type | width | default | signed range | unsigned range
bool | 1 bit | unsigned | - | 0, 1
char | 8 bits, 1 byte | signed | -128, +127 | 0, +255
short | 16 bits, 2 bytes | signed | -32.768, +32.767 | 0, +65.535
int | 16 bits, 2 bytes | signed | -32.768, +32.767 | 0, +65.535
long | 32 bits, 4 bytes | signed | -2.147.483.648, +2.147.483.647 | 0, +4.294.967.295
float | 4 bytes IEEE 754 | signed |  | 1.175494351E-38, 3.402823466E+38
pointer | 1, 2, 3 or 4 bytes | generic |  |

The compiler also allows inline assembler code to be embedded anywhere in a function. In addition, routines developed in assembly can also be called.
SDCC also provides an option (--cyclomatic) to report the relative complexity of a function. These functions can then be further optimized, or hand coded in assembly if needed.
SDCC also comes with a companion source level debugger SDCDB. The debugger currently uses ucSim, a free open source simulator for 8051 and other micro-controllers.
The latest SDCC version can be downloaded from `http://sdcc.sourceforge.net/snap.php`. Please note: the compiler will probably always be some steps ahead of this documentation 1.1.

Next: 1.2 Open Source Up: 1. Introduction Previous: 1. Introduction Contents Index