             Kaypro 16 to Kaypro 8 bit Communication



To  hard  wire  a Kaypro 16 to any of Kaypro's  8  bit  computers
follow the wire diagram below:




      5 4 3 2 1          13 12 11 10 9  8  7  6  5  4  3  2  1
     (* * * * *)        (*  *  *  *  *  *  *  *  *  *  *  *  *)
      \* * * */          \*  *  *  *  *  *  *  *  *  *  *  */
       9 8 7 6           25 24 23 22 21 20 19 18 17 16 15 14

      Kaypro 16                     Kaypro 8 bit
  Serial Modem Port               Serial Modem Port

       TX  2      <------------->      3  RX
       RX  4      <------------->      2  TX
       CTS 3      <------------->      4  RTS
       RTS 8      <------------->      5  CTS
       SG  5      <------------->      7  SG



After  you  have  connected the  two  computers,  to  communicate
between them, you need a communication software. We recommend the
program called "MITE".  Set the program in DIRECT mode,  then you
should be able to communication back and forth.


Rick Bartlett
Technical Manager
Vizden Pty. Ltd.
